https://www.sciencedirect.com/science/article/pii/S1463500319302173#!

<https://agupubs.onlinelibrary.wiley.com/doi/full/10.1029/2019JC015822>

<https://www.sciencedirect.com/science/article/pii/S0303243417301289?via%3Dihub#tbl0005>

* Use 1-D HEC-RAS
* Floodplain delineation was performed using the water surface TINs generated from the HEC-RAS simulation results and topography data to calculate the floodplain boundary and inundation depths. The floodplain is calculated where the water surface is higher than the terrain, and the inundation depth results from the rasterized water surface and terrain comparison.